Notes on VDL mode 2 MASP edits

Tom McGuffin

2023 sept 22

My notes on the common VDL mode 2 MASPS edits that I have performed since the 2023 June DLK SC meeting in Paris:

1. Removed all requirement tags

My meeting notes

Reviewed MASPS AOA paper from Boeing (tom mcguffin). See notes on AOA print out. Several times DLK wanted to delete material because it was not directly related to VDL2, such as media advisory msg logic.

Changes for AOA MASPS sections

1. ~~added dynamic N1 requirements. CMU must accept supersize AOA uplinks. CMU is not required to downlink supersize AOA blocks. Same as 618~~
2. Try to avoid negative requirements
3. Delete RAT1
4. Rewrite VAT13 logic
5. Delete most of AOA to POA switch without autotune and cleanup
6. Delete media advisory
7. Delete voice data switching
8. updated